ONX CATV and MoCA Test

The ONX CATV does not do, or connect, to a live MoCA network. Our current MoCA testing solution would be to use SmartIDs to evaluate CPE to CPE frequency responses and identify any issues that would cause degraded MoCA communications anywhere in the MoCA frequency bands (500MHz to 1.6GHz). The SmartIDs would also be helpful in determining any issues with the traditional triple play services too offered by Cable operators operating in the 2MHz to 1.2GHz frequency range.